(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 220)
    (zones 0)
    (modules 20)
    (nets 33)
  )
  (page A)
  (title_block
    (title "7th Area QSO Party Pixie Plaque")
    (date 2017-03-14)
    (rev A)
    (company "Central Oregon DX Club")
    (comment 1 "Design by Martin Held, AE7EU")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.635 0.381)
    (user_via 0.635 0.381)
    (user_via 0.889 0.635)
    (user_via 0.889 0.635)
    (user_via 1.27 0.889)
    (user_via 1.27 0.889)
    (user_via 1.905 1.524)
    (user_via 1.905 1.524)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1.27 1.27)
    (mod_text_width 0.254)
    (pad_size 0.635 0.635)
    (pad_drill 0.381)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 SCL)
  (net 3 SDA)
  (net 4 +5V)
  (net 5 "Net-(P1-Pad1)")
  (net 6 "Net-(P1-Pad2)")
  (net 7 RSTB)
  (net 8 INT1B)
  (net 9 EN1)
  (net 10 INT1A)
  (net 11 INT2B)
  (net 12 EN2)
  (net 13 INT2A)
  (net 14 INT3B)
  (net 15 EN3)
  (net 16 INT3A)
  (net 17 LED6)
  (net 18 LED5)
  (net 19 LED1)
  (net 20 LED3)
  (net 21 LED2)
  (net 22 LED4)
  (net 23 LED7)
  (net 24 LED0)
  (net 25 "Net-(P2-Pad7)")
  (net 26 "Net-(P2-Pad1)")
  (net 27 "Net-(P2-Pad3)")
  (net 28 "Net-(P2-Pad5)")
  (net 29 "Net-(P3-Pad7)")
  (net 30 "Net-(P3-Pad1)")
  (net 31 "Net-(P3-Pad3)")
  (net 32 "Net-(P3-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net EN1)
    (add_net EN2)
    (add_net EN3)
    (add_net FS)
    (add_net GND)
    (add_net INT1A)
    (add_net INT1B)
    (add_net INT2A)
    (add_net INT2B)
    (add_net INT3A)
    (add_net INT3B)
    (add_net LED0)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net LED4)
    (add_net LED5)
    (add_net LED6)
    (add_net LED7)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net RSTB)
    (add_net SCL)
    (add_net SDA)
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 35.56 82.55 180)
    (descr "SMT capacitor, 1210")
    (fp_text reference C5 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 35.56 78.74 180)
    (descr "SMT capacitor, 1210")
    (fp_text reference C4 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 35.56 74.93 180)
    (descr "SMT capacitor, 1210")
    (fp_text reference C3 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 52.07 36.83 180)
    (descr "SMT capacitor, 1210")
    (fp_text reference C2 (at 1.778 2.032 180) (layer F.SilkS))
    (fp_text value 0.1u (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 46.863 31.75 180)
    (descr "SMT capacitor, 1210")
    (fp_text reference C1 (at 1.905 2.032) (layer F.SilkS))
    (fp_text value 0.1u (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:HDR8X1_OSTVN08A150 (layer F.Cu) (tedit 5E41E90E)
    (at 67.31 66.04)
    (fp_text reference P3 (at -2.54 11.176 180) (layer F.SilkS))
    (fp_text value HDR8X1 (at -1.5 -11.1) (layer F.SilkS) hide)
    (pad 7 thru_hole circle (at 0 6.35) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(P3-Pad7)"))
    (pad 8 thru_hole circle (at 0 8.89) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0 3.81) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -8.89) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 "Net-(P3-Pad1)"))
    (pad 3 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 "Net-(P3-Pad3)"))
    (pad 2 thru_hole circle (at 0 -6.35) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 -1.27) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 1.27) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 "Net-(P3-Pad5)"))
  )
  (module mheld_std:HDR8X1_OSTVN08A150 (layer F.Cu) (tedit 5E41E90E)
    (at 67.31 44.45)
    (fp_text reference P2 (at -2.54 -11.176 180) (layer F.SilkS))
    (fp_text value HDR8X1 (at -1.5 -11.1) (layer F.SilkS) hide)
    (pad 7 thru_hole circle (at 0 6.35) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad7)"))
    (pad 8 thru_hole circle (at 0 8.89) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 0 3.81) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 -8.89) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad1)"))
    (pad 3 thru_hole circle (at 0 -3.81) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad3)"))
    (pad 2 thru_hole circle (at 0 -6.35) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 -1.27) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 1.27) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad5)"))
  )
  (module mheld_std:TEENSY31_Basic (layer F.Cu) (tedit 5E41A482)
    (at 27.051 34.544)
    (descr Teensy31)
    (fp_text reference U1 (at 0.889 -0.9144 180) (layer F.SilkS))
    (fp_text value TEENSY31 (at 12.0396 -0.9398 180) (layer F.SilkS) hide)
    (pad 33 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 32 thru_hole circle (at 16.51 3.81) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at 16.51 6.35) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 9 EN1))
    (pad 30 thru_hole circle (at 16.51 8.89) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 10 INT1A))
    (pad 29 thru_hole circle (at 16.51 11.43) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 8 INT1B))
    (pad 28 thru_hole circle (at 16.51 13.97) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 17 LED6))
    (pad 27 thru_hole circle (at 16.51 16.51) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 18 LED5))
    (pad 26 thru_hole circle (at 16.51 19.05) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 25 thru_hole circle (at 16.51 21.59) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 24 thru_hole circle (at 16.51 24.13) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 7 RSTB))
    (pad 23 thru_hole circle (at 16.51 26.67) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 13 INT2A))
    (pad 22 thru_hole circle (at 16.51 29.21) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 11 INT2B))
    (pad 21 thru_hole circle (at 16.51 31.75) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 19 LED1))
    (pad 20 thru_hole circle (at 16.51 34.29) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 12 EN2))
    (pad 17 thru_hole circle (at 8.89 34.29) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at 1.27 34.29) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 14 INT3B))
    (pad 13 thru_hole circle (at 1.27 31.75) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 16 INT3A))
    (pad 12 thru_hole circle (at 1.27 29.21) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 1.27 26.67) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 15 EN3))
    (pad 10 thru_hole circle (at 1.27 24.13) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 20 LED3))
    (pad 9 thru_hole circle (at 1.27 21.59) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 21 LED2))
    (pad 8 thru_hole circle (at 1.27 19.05) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 22 LED4))
    (pad 7 thru_hole circle (at 1.27 16.51) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 23 LED7))
    (pad 6 thru_hole circle (at 1.27 13.97) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.27 11.43) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 1.27 8.89) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 24 LED0))
    (pad 3 thru_hole circle (at 1.27 6.35) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 1.27) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:HDR2X1_P1 (layer F.Cu) (tedit 5407816B)
    (at 45.72 27.94 90)
    (fp_text reference P13 (at 1.905 -0.254) (layer F.SilkS))
    (fp_text value HDR2X1 (at 0.47 -1.94 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 +5V))
  )
  (module mheld_std:DIP-20_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 48.788 40.64)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at -0.274 -2.032) (layer F.SilkS))
    (fp_text value 74HCT245 (at 3.81 25.19) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 LED1))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(P2-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 LED3))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 LED2))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 LED4))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad7)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 LED7))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(P3-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 LED5))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(P3-Pad3)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 LED6))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(P3-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 LED0))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(P3-Pad7)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R1210 (layer F.Cu) (tedit 5407975A)
    (at 40.64 52.07 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference R2 (at 3.302 0 180) (layer F.SilkS))
    (fp_text value 10k (at -0.0254 1.7272 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 2 SCL))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model smd/resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R1210 (layer F.Cu) (tedit 5407975A)
    (at 35.56 52.07 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference R1 (at 3.302 0 180) (layer F.SilkS))
    (fp_text value 10k (at -0.0254 1.7272 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 3 SDA))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model smd/resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:HDR8X1_P1 (layer F.Cu) (tedit 54077F6D)
    (at 57.15 82.55 270)
    (fp_text reference P12 (at 0 -2.54) (layer F.SilkS))
    (fp_text value HDR8X1 (at 0.47 -1.94 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 RSTB))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 INT3B))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 EN3))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 INT3A))
    (pad 7 thru_hole circle (at 0 15.24 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 17.78 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 6 thru_hole circle (at 0 12.7 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 SDA))
  )
  (module mheld_std:HDR8X1_P1 (layer F.Cu) (tedit 54077F6D)
    (at 57.15 78.74 270)
    (fp_text reference P11 (at 0 -2.54) (layer F.SilkS))
    (fp_text value HDR8X1 (at 0.47 -1.94 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 RSTB))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 INT2B))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 EN2))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 INT2A))
    (pad 7 thru_hole circle (at 0 15.24 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 17.78 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 6 thru_hole circle (at 0 12.7 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 SDA))
  )
  (module mheld_std:HDR2X1_P1 (layer F.Cu) (tedit 5407816B)
    (at 38.1 33.02 270)
    (fp_text reference P1 (at -2.032 3.048) (layer F.SilkS))
    (fp_text value HDR2X1 (at 0.47 -1.94 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad2)"))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 67.31 81.28)
    (fp_text reference TH4 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 67.31 29.21)
    (fp_text reference TH3 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 29.21 29.21)
    (fp_text reference TH2 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 29.21 81.28)
    (fp_text reference TH1 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:HDR8X1_P1 (layer F.Cu) (tedit 54077F6D)
    (at 57.15 74.93 270)
    (fp_text reference P10 (at 0 -2.54) (layer F.SilkS))
    (fp_text value HDR8X1 (at 0.47 -1.94 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 RSTB))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 8 INT1B))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 9 EN1))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 10 INT1A))
    (pad 7 thru_hole circle (at 0 15.24 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 17.78 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 6 thru_hole circle (at 0 12.7 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 SDA))
  )
  (gr_text ae7eu.com/decay/ (at 47.244 70.866) (layer B.SilkS))
  (gr_text "LED4\n\nGND\n\nLED2\n\nGND\n\nLED3\n\nGND\n\nLED1\n\nGND\n" (at 63.5 66.04) (layer F.SilkS))
  (gr_text "LED0\n\nGND\n\nLED6\n\nGND\n\nLED5\n\nGND\n\nLED7\n\nGND\n" (at 63.5 44.45) (layer F.SilkS))
  (gr_text GND (at 41.91 27.94) (layer F.SilkS))
  (gr_text +5V (at 51.943 27.94) (layer F.SilkS))
  (gr_text "martin.held@gmail.com\nMartin Held, AE7EU\nThe Decay of Art\nMain Controller" (at 52.578 33.782) (layer B.SilkS))
  (gr_text "+5V\n\nGND\n\nSCL\n\nSDA\n\nEN\n\nINTA\n\nINTB\n\nRST" (at 48.26 73.66 90) (layer F.SilkS))
  (dimension 22.86 (width 0.15) (layer Dwgs.User)
    (gr_text "0.9000 in" (at 36.83 22.83) (layer Dwgs.User))
    (feature1 (pts (xy 48.26 25.4) (xy 48.26 23.543579)))
    (feature2 (pts (xy 25.4 25.4) (xy 25.4 23.543579)))
    (crossbar (pts (xy 25.4 24.13) (xy 48.26 24.13)))
    (arrow1a (pts (xy 48.26 24.13) (xy 47.133496 24.716421)))
    (arrow1b (pts (xy 48.26 24.13) (xy 47.133496 23.543579)))
    (arrow2a (pts (xy 25.4 24.13) (xy 26.526504 24.716421)))
    (arrow2b (pts (xy 25.4 24.13) (xy 26.526504 23.543579)))
  )
  (dimension 53.34 (width 0.15) (layer Dwgs.User)
    (gr_text "2.1000 in" (at 81.31 52.07 270) (layer Dwgs.User))
    (feature1 (pts (xy 71.12 78.74) (xy 80.596421 78.74)))
    (feature2 (pts (xy 71.12 25.4) (xy 80.596421 25.4)))
    (crossbar (pts (xy 80.01 25.4) (xy 80.01 78.74)))
    (arrow1a (pts (xy 80.01 78.74) (xy 79.423579 77.613496)))
    (arrow1b (pts (xy 80.01 78.74) (xy 80.596421 77.613496)))
    (arrow2a (pts (xy 80.01 25.4) (xy 79.423579 26.526504)))
    (arrow2b (pts (xy 80.01 25.4) (xy 80.596421 26.526504)))
  )
  (dimension 45.72 (width 0.15) (layer Dwgs.User)
    (gr_text "1.8000 in" (at 48.26 21.56) (layer Dwgs.User))
    (feature1 (pts (xy 71.12 25.4) (xy 71.12 22.273579)))
    (feature2 (pts (xy 25.4 25.4) (xy 25.4 22.273579)))
    (crossbar (pts (xy 25.4 22.86) (xy 71.12 22.86)))
    (arrow1a (pts (xy 71.12 22.86) (xy 69.993496 23.446421)))
    (arrow1b (pts (xy 71.12 22.86) (xy 69.993496 22.273579)))
    (arrow2a (pts (xy 25.4 22.86) (xy 26.526504 23.446421)))
    (arrow2b (pts (xy 25.4 22.86) (xy 26.526504 22.273579)))
  )
  (gr_line (start 25.4 85.09) (end 25.4 25.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 85.09) (end 25.4 85.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 25.4) (end 71.12 85.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 25.4 25.4) (end 71.12 25.4) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 25.4 25.4) (xy 71.12 25.4) (xy 71.12 85.09) (xy 25.4 85.09)
      )
    )
  )
)
