(kicad_pcb (version 20171130) (host pcbnew 5.1.0-060a0da~80~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 474)
    (zones 0)
    (modules 33)
    (nets 94)
  )
  (page A)
  (title_block
    (title "7th Area QSO Party Pixie Plaque")
    (date 2017-03-14)
    (rev A)
    (company "Central Oregon DX Club")
    (comment 1 "Design by Martin Held, AE7EU")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.635 0.381)
    (user_via 0.635 0.381)
    (user_via 0.889 0.635)
    (user_via 0.889 0.635)
    (user_via 1.27 0.889)
    (user_via 1.27 0.889)
    (user_via 1.905 1.524)
    (user_via 1.905 1.524)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1.27 1.27)
    (mod_text_width 0.254)
    (pad_size 0.635 0.635)
    (pad_drill 0.381)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P4-Pad1)")
  (net 3 "Net-(P5-Pad2)")
  (net 4 SCL)
  (net 5 SDA)
  (net 6 "Net-(C8-Pad1)")
  (net 7 +5V)
  (net 8 "Net-(C3-Pad1)")
  (net 9 "Net-(C5-Pad1)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 "Net-(P1-Pad1)")
  (net 12 "Net-(P1-Pad2)")
  (net 13 "Net-(P1-Pad4)")
  (net 14 "Net-(P1-Pad3)")
  (net 15 "Net-(P1-Pad7)")
  (net 16 "Net-(P1-Pad8)")
  (net 17 "Net-(P1-Pad6)")
  (net 18 "Net-(P1-Pad5)")
  (net 19 "Net-(P1-Pad10)")
  (net 20 "Net-(P1-Pad9)")
  (net 21 RSTB)
  (net 22 INTB)
  (net 23 /EN)
  (net 24 INTA)
  (net 25 "Net-(P2-Pad5)")
  (net 26 "Net-(P3-Pad1)")
  (net 27 "Net-(P3-Pad2)")
  (net 28 "Net-(P3-Pad4)")
  (net 29 "Net-(P3-Pad3)")
  (net 30 "Net-(P3-Pad7)")
  (net 31 "Net-(P3-Pad8)")
  (net 32 "Net-(P3-Pad6)")
  (net 33 "Net-(P3-Pad5)")
  (net 34 "Net-(P3-Pad10)")
  (net 35 "Net-(P3-Pad9)")
  (net 36 "Net-(P4-Pad2)")
  (net 37 "Net-(P4-Pad4)")
  (net 38 "Net-(P4-Pad3)")
  (net 39 "Net-(P4-Pad7)")
  (net 40 "Net-(P4-Pad8)")
  (net 41 "Net-(P4-Pad6)")
  (net 42 "Net-(P4-Pad5)")
  (net 43 "Net-(P4-Pad10)")
  (net 44 "Net-(P4-Pad9)")
  (net 45 "Net-(P5-Pad1)")
  (net 46 "Net-(P5-Pad4)")
  (net 47 "Net-(P5-Pad3)")
  (net 48 "Net-(P5-Pad7)")
  (net 49 "Net-(P5-Pad8)")
  (net 50 "Net-(P5-Pad6)")
  (net 51 "Net-(P5-Pad5)")
  (net 52 "Net-(P5-Pad10)")
  (net 53 "Net-(P5-Pad9)")
  (net 54 "Net-(R3-Pad5)")
  (net 55 "Net-(R3-Pad6)")
  (net 56 "Net-(R3-Pad7)")
  (net 57 "Net-(R3-Pad8)")
  (net 58 "Net-(R4-Pad5)")
  (net 59 "Net-(R4-Pad6)")
  (net 60 "Net-(R4-Pad7)")
  (net 61 "Net-(R4-Pad8)")
  (net 62 "Net-(R5-Pad5)")
  (net 63 "Net-(R5-Pad6)")
  (net 64 "Net-(R5-Pad7)")
  (net 65 "Net-(R5-Pad8)")
  (net 66 "Net-(R6-Pad5)")
  (net 67 "Net-(R6-Pad6)")
  (net 68 "Net-(R6-Pad7)")
  (net 69 "Net-(R6-Pad8)")
  (net 70 "Net-(R7-Pad5)")
  (net 71 "Net-(R7-Pad6)")
  (net 72 "Net-(R7-Pad7)")
  (net 73 "Net-(R7-Pad8)")
  (net 74 "Net-(R8-Pad5)")
  (net 75 "Net-(R8-Pad6)")
  (net 76 "Net-(R8-Pad7)")
  (net 77 "Net-(R8-Pad8)")
  (net 78 "Net-(R9-Pad5)")
  (net 79 "Net-(R9-Pad6)")
  (net 80 "Net-(R9-Pad7)")
  (net 81 "Net-(R9-Pad8)")
  (net 82 "Net-(R10-Pad5)")
  (net 83 "Net-(R10-Pad6)")
  (net 84 "Net-(R10-Pad7)")
  (net 85 "Net-(R10-Pad8)")
  (net 86 "Net-(R11-Pad5)")
  (net 87 "Net-(R11-Pad6)")
  (net 88 "Net-(R11-Pad7)")
  (net 89 "Net-(R11-Pad8)")
  (net 90 "Net-(R12-Pad5)")
  (net 91 "Net-(R12-Pad6)")
  (net 92 "Net-(R12-Pad7)")
  (net 93 "Net-(R12-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /EN)
    (add_net GND)
    (add_net INTA)
    (add_net INTB)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad10)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P4-Pad6)")
    (add_net "Net-(P4-Pad7)")
    (add_net "Net-(P4-Pad8)")
    (add_net "Net-(P4-Pad9)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad10)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(P5-Pad5)")
    (add_net "Net-(P5-Pad6)")
    (add_net "Net-(P5-Pad7)")
    (add_net "Net-(P5-Pad8)")
    (add_net "Net-(P5-Pad9)")
    (add_net "Net-(R10-Pad5)")
    (add_net "Net-(R10-Pad6)")
    (add_net "Net-(R10-Pad7)")
    (add_net "Net-(R10-Pad8)")
    (add_net "Net-(R11-Pad5)")
    (add_net "Net-(R11-Pad6)")
    (add_net "Net-(R11-Pad7)")
    (add_net "Net-(R11-Pad8)")
    (add_net "Net-(R12-Pad5)")
    (add_net "Net-(R12-Pad6)")
    (add_net "Net-(R12-Pad7)")
    (add_net "Net-(R12-Pad8)")
    (add_net "Net-(R3-Pad5)")
    (add_net "Net-(R3-Pad6)")
    (add_net "Net-(R3-Pad7)")
    (add_net "Net-(R3-Pad8)")
    (add_net "Net-(R4-Pad5)")
    (add_net "Net-(R4-Pad6)")
    (add_net "Net-(R4-Pad7)")
    (add_net "Net-(R4-Pad8)")
    (add_net "Net-(R5-Pad5)")
    (add_net "Net-(R5-Pad6)")
    (add_net "Net-(R5-Pad7)")
    (add_net "Net-(R5-Pad8)")
    (add_net "Net-(R6-Pad5)")
    (add_net "Net-(R6-Pad6)")
    (add_net "Net-(R6-Pad7)")
    (add_net "Net-(R6-Pad8)")
    (add_net "Net-(R7-Pad5)")
    (add_net "Net-(R7-Pad6)")
    (add_net "Net-(R7-Pad7)")
    (add_net "Net-(R7-Pad8)")
    (add_net "Net-(R8-Pad5)")
    (add_net "Net-(R8-Pad6)")
    (add_net "Net-(R8-Pad7)")
    (add_net "Net-(R8-Pad8)")
    (add_net "Net-(R9-Pad5)")
    (add_net "Net-(R9-Pad6)")
    (add_net "Net-(R9-Pad7)")
    (add_net "Net-(R9-Pad8)")
    (add_net RSTB)
    (add_net SCL)
    (add_net SDA)
  )
  (module mheld_std:SSOP-A32 (layer F.Cu) (tedit 5E3E37E8)
    (at 55.88 52.07)
    (attr smd)
    (fp_text reference U3 (at -6.096 -5.08 180) (layer F.SilkS))
    (fp_text value BU21182 (at 0 0) (layer F.SilkS))
    (pad 16 smd rect (at 6 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R11-Pad5)"))
    (pad 17 smd rect (at 6 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R10-Pad8)"))
    (pad 15 smd rect (at 5.2 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(R11-Pad6)"))
    (pad 18 smd rect (at 5.2 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R10-Pad7)"))
    (pad 14 smd rect (at 4.4 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(R11-Pad7)"))
    (pad 19 smd rect (at 4.4 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R10-Pad6)"))
    (pad 13 smd rect (at 3.6 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(R11-Pad8)"))
    (pad 20 smd rect (at 3.6 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R10-Pad5)"))
    (pad 12 smd rect (at 2.8 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(R12-Pad5)"))
    (pad 21 smd rect (at 2.8 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(R9-Pad8)"))
    (pad 11 smd rect (at 2 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R12-Pad6)"))
    (pad 22 smd rect (at 2 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R9-Pad7)"))
    (pad 10 smd rect (at 1.2 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(R12-Pad7)"))
    (pad 23 smd rect (at 1.2 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R9-Pad6)"))
    (pad 9 smd rect (at 0.4 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R12-Pad8)"))
    (pad 24 smd rect (at 0.4 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R9-Pad5)"))
    (pad 8 smd rect (at -0.4 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -0.4 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R8-Pad8)"))
    (pad 7 smd rect (at -1.2 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -1.2 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(R8-Pad7)"))
    (pad 6 smd rect (at -2 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 27 smd rect (at -2 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(R8-Pad6)"))
    (pad 5 smd rect (at -2.8 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 RSTB))
    (pad 28 smd rect (at -2.8 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R8-Pad5)"))
    (pad 4 smd rect (at -3.6 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 INTB))
    (pad 29 smd rect (at -3.6 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (pad 3 smd rect (at -4.4 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL))
    (pad 30 smd rect (at -4.4 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -5.2 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA))
    (pad 31 smd rect (at -5.2 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -6 3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -6 -3.6) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
  )
  (module mheld_std:SOT25 (layer F.Cu) (tedit 54C19F0A)
    (at 46.99 33.02)
    (descr SOT23)
    (attr smd)
    (fp_text reference U2 (at -2.54 0) (layer F.SilkS))
    (fp_text value NC7SZ384 (at -0.508 3.048) (layer F.SilkS))
    (pad 3 smd rect (at 0.9525 1.3081) (size 0.59944 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 1.31064) (size 0.59944 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA))
    (pad 1 smd rect (at -0.9525 1.31064) (size 0.59944 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P2-Pad5)"))
    (pad 4 smd rect (at 0.9525 -1.31064) (size 0.59944 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 23 /EN))
    (pad 5 smd rect (at -0.9525 -1.31064) (size 0.59944 1.2192) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (model smd/smd_transistors/sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SSOP-A32 (layer F.Cu) (tedit 5E3E37E8)
    (at 40.64 52.07 180)
    (attr smd)
    (fp_text reference U1 (at 5.842 5.08) (layer F.SilkS))
    (fp_text value BU21182 (at 0 0 180) (layer F.SilkS))
    (pad 16 smd rect (at 6 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R6-Pad5)"))
    (pad 17 smd rect (at 6 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R5-Pad8)"))
    (pad 15 smd rect (at 5.2 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R6-Pad6)"))
    (pad 18 smd rect (at 5.2 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R5-Pad7)"))
    (pad 14 smd rect (at 4.4 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R6-Pad7)"))
    (pad 19 smd rect (at 4.4 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R5-Pad6)"))
    (pad 13 smd rect (at 3.6 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R6-Pad8)"))
    (pad 20 smd rect (at 3.6 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R5-Pad5)"))
    (pad 12 smd rect (at 2.8 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R7-Pad5)"))
    (pad 21 smd rect (at 2.8 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R4-Pad8)"))
    (pad 11 smd rect (at 2 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R7-Pad6)"))
    (pad 22 smd rect (at 2 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R4-Pad7)"))
    (pad 10 smd rect (at 1.2 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R7-Pad7)"))
    (pad 23 smd rect (at 1.2 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R4-Pad6)"))
    (pad 9 smd rect (at 0.4 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R7-Pad8)"))
    (pad 24 smd rect (at 0.4 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R4-Pad5)"))
    (pad 8 smd rect (at -0.4 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 25 smd rect (at -0.4 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R3-Pad8)"))
    (pad 7 smd rect (at -1.2 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -1.2 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R3-Pad7)"))
    (pad 6 smd rect (at -2 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at -2 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R3-Pad6)"))
    (pad 5 smd rect (at -2.8 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 RSTB))
    (pad 28 smd rect (at -2.8 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R3-Pad5)"))
    (pad 4 smd rect (at -3.6 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 INTA))
    (pad 29 smd rect (at -3.6 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -4.4 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL))
    (pad 30 smd rect (at -4.4 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -5.2 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA))
    (pad 31 smd rect (at -5.2 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -6 3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 32 smd rect (at -6 -3.6 180) (size 0.5 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 63.5 74.93)
    (fp_text reference TH4 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 63.5 29.21)
    (fp_text reference TH3 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 33.02 29.21)
    (fp_text reference TH2 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BE0DB17)
    (at 33.02 74.93)
    (fp_text reference TH1 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 64.77 69.85 90)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R12 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(R12-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(R12-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(R12-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R12-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P5-Pad4)"))
    (pad 3 smd rect (at 0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P5-Pad3)"))
    (pad 2 smd rect (at -0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P5-Pad2)"))
    (pad 1 smd rect (at -1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(P5-Pad1)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 64.77 62.23 90)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R11 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R11-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(R11-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(R11-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(R11-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(P5-Pad8)"))
    (pad 3 smd rect (at 0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P5-Pad7)"))
    (pad 2 smd rect (at -0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(P5-Pad6)"))
    (pad 1 smd rect (at -1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(P5-Pad5)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 64.77 52.07 90)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R10 (at 2.54 0) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R10-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R10-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R10-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(R10-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P4-Pad2)"))
    (pad 3 smd rect (at 0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at -0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P5-Pad10)"))
    (pad 1 smd rect (at -1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(P5-Pad9)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 64.77 41.91 90)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R9 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(R9-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(R9-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(R9-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(R9-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P4-Pad6)"))
    (pad 3 smd rect (at 0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P4-Pad5)"))
    (pad 2 smd rect (at -0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P4-Pad4)"))
    (pad 1 smd rect (at -1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(P4-Pad3)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 64.77 34.29 90)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R8 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R8-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(R8-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(R8-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R8-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P4-Pad10)"))
    (pad 3 smd rect (at 0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(P4-Pad9)"))
    (pad 2 smd rect (at -0.40005 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(P4-Pad8)"))
    (pad 1 smd rect (at -1.20015 0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(P4-Pad7)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 31.75 34.29 270)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R7 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 270) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(R7-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R7-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R7-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R7-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P3-Pad4)"))
    (pad 3 smd rect (at 0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P3-Pad3)"))
    (pad 2 smd rect (at -0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P3-Pad2)"))
    (pad 1 smd rect (at -1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P3-Pad1)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 31.75 41.91 270)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R6 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 270) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R6-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R6-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R6-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R6-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P3-Pad8)"))
    (pad 3 smd rect (at 0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P3-Pad7)"))
    (pad 2 smd rect (at -0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P3-Pad6)"))
    (pad 1 smd rect (at -1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P3-Pad5)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 31.75 52.07 270)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R5 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 270) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R5-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(R5-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R5-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R5-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at -0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P3-Pad10)"))
    (pad 1 smd rect (at -1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P3-Pad9)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 31.75 62.23 270)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R4 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 270) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R4-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R4-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R4-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R4-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P1-Pad6)"))
    (pad 3 smd rect (at 0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P1-Pad5)"))
    (pad 2 smd rect (at -0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad4)"))
    (pad 1 smd rect (at -1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P1-Pad3)"))
  )
  (module mheld_std:CRA06E (layer F.Cu) (tedit 563BFAA6)
    (at 31.75 69.85 270)
    (descr "Surface mount Resistor netowrk, vishay dale cra06es")
    (fp_text reference R3 (at 0 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at 4.064 0 270) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R3-Pad5)"))
    (pad 6 smd rect (at 0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R3-Pad6)"))
    (pad 7 smd rect (at -0.40005 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(R3-Pad7)"))
    (pad 8 smd rect (at -1.20015 -0.974979) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(R3-Pad8)"))
    (pad 4 smd rect (at 1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P1-Pad10)"))
    (pad 3 smd rect (at 0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad9)"))
    (pad 2 smd rect (at -0.40005 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P1-Pad8)"))
    (pad 1 smd rect (at -1.20015 0.974979 180) (size 1.149858 0.439928) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P1-Pad7)"))
  )
  (module mheld_std:R1210 (layer F.Cu) (tedit 5407975A)
    (at 40.64 35.56 180)
    (descr "SMT capacitor, 1210")
    (fp_text reference R2 (at 3.048 0.254 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 SCL))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (model smd/resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:R1210 (layer F.Cu) (tedit 5407975A)
    (at 50.8 33.02 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference R1 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 10k (at -0.0254 0.254 180) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (model smd/resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:HDR10X1_P1 (layer F.Cu) (tedit 5407747A)
    (at 68.58 76.2 180)
    (fp_text reference P5 (at 2.54 19.05) (layer F.SilkS))
    (fp_text value HDR10X1 (at 0.47 -1.94 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 45 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 3 "Net-(P5-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 46 "Net-(P5-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 47 "Net-(P5-Pad3)"))
    (pad 7 thru_hole circle (at 0 15.24 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 48 "Net-(P5-Pad7)"))
    (pad 8 thru_hole circle (at 0 17.78 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 49 "Net-(P5-Pad8)"))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 50 "Net-(P5-Pad6)"))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 51 "Net-(P5-Pad5)"))
    (pad 10 thru_hole circle (at 0 22.86 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 52 "Net-(P5-Pad10)"))
    (pad 9 thru_hole circle (at 0 20.32 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 53 "Net-(P5-Pad9)"))
  )
  (module mheld_std:HDR10X1_P1 (layer F.Cu) (tedit 5407747A)
    (at 68.58 50.8 180)
    (fp_text reference P4 (at 2.54 3.81) (layer F.SilkS))
    (fp_text value HDR10X1 (at 0.47 -1.94 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 2 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 36 "Net-(P4-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 37 "Net-(P4-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 38 "Net-(P4-Pad3)"))
    (pad 7 thru_hole circle (at 0 15.24 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 39 "Net-(P4-Pad7)"))
    (pad 8 thru_hole circle (at 0 17.78 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 40 "Net-(P4-Pad8)"))
    (pad 6 thru_hole circle (at 0 12.7 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 41 "Net-(P4-Pad6)"))
    (pad 5 thru_hole circle (at 0 10.16 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 42 "Net-(P4-Pad5)"))
    (pad 10 thru_hole circle (at 0 22.86 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 43 "Net-(P4-Pad10)"))
    (pad 9 thru_hole circle (at 0 20.32 180) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 44 "Net-(P4-Pad9)"))
  )
  (module mheld_std:HDR10X1_P1 (layer F.Cu) (tedit 5407747A)
    (at 27.94 27.94)
    (fp_text reference P3 (at 2.54 19.05 180) (layer F.SilkS))
    (fp_text value HDR10X1 (at 0.47 -1.94) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 26 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 27 "Net-(P3-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 28 "Net-(P3-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 29 "Net-(P3-Pad3)"))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 30 "Net-(P3-Pad7)"))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 31 "Net-(P3-Pad8)"))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 32 "Net-(P3-Pad6)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad5)"))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 34 "Net-(P3-Pad10)"))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 35 "Net-(P3-Pad9)"))
  )
  (module mheld_std:HDR8X1_P1 (layer F.Cu) (tedit 54077F6D)
    (at 57.15 29.21 270)
    (fp_text reference P2 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value HDR8X1 (at 0.47 -1.94 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 21 RSTB))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 22 INTB))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 /EN))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 24 INTA))
    (pad 7 thru_hole circle (at 0 15.24 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 0 17.78 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 6 thru_hole circle (at 0 12.7 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 25 "Net-(P2-Pad5)"))
  )
  (module mheld_std:HDR10X1_P1 (layer F.Cu) (tedit 5407747A)
    (at 27.94 53.34)
    (fp_text reference P1 (at 2.286 3.81 180) (layer F.SilkS))
    (fp_text value HDR10X1 (at 0.47 -1.94) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad3)"))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad7)"))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad8)"))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad6)"))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad5)"))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 19 "Net-(P1-Pad10)"))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 20 "Net-(P1-Pad9)"))
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 45.212 42.164 270)
    (descr "SMT capacitor, 1210")
    (fp_text reference C9 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 1.0u (at 0 0) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 54.356 42.164 270)
    (descr "SMT capacitor, 1210")
    (fp_text reference C8 (at -3.048 0) (layer F.SilkS))
    (fp_text value 2.2u (at -0.0254 0) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C8-Pad1)"))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 48.26 42.164 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference C7 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 180) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 51.308 42.164 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference C6 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 0 180) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 52.578 60.96 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference C5 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 1.0u (at -0.0254 0 180) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C5-Pad1)"))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 40.64 32.512)
    (descr "SMT capacitor, 1210")
    (fp_text reference C4 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0 90) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 1 smd rect (at 1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 43.434 60.96 90)
    (descr "SMT capacitor, 1210")
    (fp_text reference C3 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 2.2u (at -0.0254 0 180) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C3-Pad1)"))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 46.482 60.96 270)
    (descr "SMT capacitor, 1210")
    (fp_text reference C2 (at 3.048 0) (layer F.SilkS))
    (fp_text value 0.1u (at 0 0) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 1 smd rect (at 1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 49.53 60.96 270)
    (descr "SMT capacitor, 1210")
    (fp_text reference C1 (at 3.048 0) (layer F.SilkS))
    (fp_text value 4.7u (at 0 0) (layer F.SilkS))
    (pad 2 smd rect (at -1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 1 smd rect (at 1.397 0 270) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "R3-R12: Value TBD" (at 59.436 39.37 90) (layer F.SilkS))
  (gr_text "OH BABY\n\nTOUCH ME" (at 48.26 49.022) (layer B.SilkS))
  (gr_text "+5V\n\nGND\n\nSCL\n\nSDA\n\nEN\n\nINTA\n\nINTB\n\nRST" (at 48.26 27.94 90) (layer F.SilkS))
  (gr_text "martin.held@gmail.com\nMartin Held, AE7EU\nThe Decay of Art\n40-Ch Touch Sensor\nae7eu.com/decay/" (at 48.26 72.39) (layer F.SilkS))
  (dimension 22.86 (width 0.15) (layer Dwgs.User)
    (gr_text "0.9000 in" (at 36.83 22.83) (layer Dwgs.User))
    (feature1 (pts (xy 48.26 25.4) (xy 48.26 23.543579)))
    (feature2 (pts (xy 25.4 25.4) (xy 25.4 23.543579)))
    (crossbar (pts (xy 25.4 24.13) (xy 48.26 24.13)))
    (arrow1a (pts (xy 48.26 24.13) (xy 47.133496 24.716421)))
    (arrow1b (pts (xy 48.26 24.13) (xy 47.133496 23.543579)))
    (arrow2a (pts (xy 25.4 24.13) (xy 26.526504 24.716421)))
    (arrow2b (pts (xy 25.4 24.13) (xy 26.526504 23.543579)))
  )
  (dimension 53.34 (width 0.15) (layer Dwgs.User)
    (gr_text "2.1000 in" (at 81.31 52.07 270) (layer Dwgs.User))
    (feature1 (pts (xy 71.12 78.74) (xy 80.596421 78.74)))
    (feature2 (pts (xy 71.12 25.4) (xy 80.596421 25.4)))
    (crossbar (pts (xy 80.01 25.4) (xy 80.01 78.74)))
    (arrow1a (pts (xy 80.01 78.74) (xy 79.423579 77.613496)))
    (arrow1b (pts (xy 80.01 78.74) (xy 80.596421 77.613496)))
    (arrow2a (pts (xy 80.01 25.4) (xy 79.423579 26.526504)))
    (arrow2b (pts (xy 80.01 25.4) (xy 80.596421 26.526504)))
  )
  (dimension 45.72 (width 0.15) (layer Dwgs.User)
    (gr_text "1.8000 in" (at 48.26 21.56) (layer Dwgs.User))
    (feature1 (pts (xy 71.12 25.4) (xy 71.12 22.273579)))
    (feature2 (pts (xy 25.4 25.4) (xy 25.4 22.273579)))
    (crossbar (pts (xy 25.4 22.86) (xy 71.12 22.86)))
    (arrow1a (pts (xy 71.12 22.86) (xy 69.993496 23.446421)))
    (arrow1b (pts (xy 71.12 22.86) (xy 69.993496 22.273579)))
    (arrow2a (pts (xy 25.4 22.86) (xy 26.526504 23.446421)))
    (arrow2b (pts (xy 25.4 22.86) (xy 26.526504 22.273579)))
  )
  (gr_line (start 25.4 78.74) (end 25.4 25.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 78.74) (end 25.4 78.74) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 71.12 25.4) (end 71.12 78.74) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 25.4 25.4) (end 71.12 25.4) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25.4 25.4) (xy 71.12 25.4) (xy 71.12 78.74) (xy 25.4 78.74)
      )
    )
  )
)
